
[](http://www.bhphotovideo.com/bnh/controller/home?O=ProductDetail&A=showItemLargeImage&Q=&sku=391552&is=REG)Samsung Digital Presenter   
~ The Basics ~


2 Options

1. Connect directly to your projector using the VGA Cable
   1. Turn on the Digital Presenter
   2. Select the right source on the projector
   3. Your image should now be on the screen.
2. Run through your computer using the USB cable and provided software. (This option takes software installation and is only available with one time help from the ITS.)

Samsung Digital Presenter – The Software

Before getting started the software must have been loaded by your ITS.

1. Connect the camera via USB cable. *Note: The same USB port must be used each time you connect the camera.*
2. Turn on the Digital Presenter
3. Open the software by clicking on the icon on the desktop. *Note: If you open the software before the camera is connected and on you will get an error message. Sometimes this means rebooting your computer to get the software to work.*



**Options: Change the location of Q-Save files.**

**Changes the Screen size of the Projector**

**Esc – Will exit from Full Screen Mode**


**Saves the image on the screen as a jpg image.**

**Change save location in Options**

**Control Panel – opens the side control panel for more options.**

**Exit – Closes the Digital Presenter program.**

1. **Overview of the View Panel**
2. **Control Panel** – Some of the same buttons are on your remote and on the base of the camera.



**Wide/Tele** - Zooms image in and out

**Focus -** Near/Far

**AF –** Auto Focus

**AWC –** Auto Adjust the Color

**Turns the Lamp on the camera on and off.**

**Negative** – change image between Negative and positive

**Aperture** – Switch between image and text mode


Digital Function is not available on this model.

**Capture –** Freezes the image on the screen – also preps it for saving and printing.

**Save –** Saves the image that has been captured as a jpg file.

**Print –** Sends the image that has been captured to the printer.

**DIP** – Digital Image Panel – Allows for customization of the image

Making Movies

1. Make sure the SDP View Panel Program is closed.
2. Go to Start – All Programs – SDP850DX USB Viewer - SDP850DX AVI Capture
3. Adjust the image with the control on the screen.
4. An external microphone must be used on desktops to capture sound. Laptops have built in microphones.
5. Click Capture to begin recording and select your network folder to save the movie.
6. Click Stop to finish recording.
7. Click Exit to end the program.
8. Movies can be edited in MovieMaker.